#### 7.2.4.12 Pset_SwitchingDeviceTypeSelectorSwitch

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / SELECTORSWITCH

| A selector switch is a switch that adjusts electrical power through a multi-position action. HISTORY: Added in IFC4.
| 切替えスイッチは複数のポジションに合わせることで電力を調整するスイッチである。 履歴： IFC4に追加。

buildingSMART Data Dictionary

PSD-XML

- SelectorType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchingDeviceDimmerSwitchType: BUTTONS, SLIDE, TWIST, OTHER, NOTKNOWN, UNSET

  | SelectorType: A list of the available types of selector switch from which that required may be selected.
  | セレクター（スイッチ）タイプ: 選択が必要となる、切替えスイッチの一覧リスト。
  | 스위치 타입: 전환스위치 목록

- SwitchUsage
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchUsage: EMERGENCY, GUARD, LIMIT, START, STOP, OTHER, NOTKNOWN, UNSET

  | SwitchUsage: A list of the available usages for selector switches from which that required may be selected.
  | スイッチの使用法: 選択が必要となる、切替えスイッチの使用法の一覧リスト。
  | 스위치 사용: 전환스위치 사용 목록

- SwitchActivation
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchActivation: ACTUATOR, FOOT, HAND, PROXIMITY, SOUND, TWOHAND, WIRE, OTHER, NOTKNOWN, UNSET

  | SwitchActivation: A list of the available activations for selector switches from which that required may be selected.
  | 起動方式: 選択が必要となる、切替えスイッチの起動方式の一覧リスト。
  | 기동 방식: 스위치 부팅방식의 목록

Link to this page