#### 7.1.4.30 Pset_SensorTypeIonConcentrationSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / IONCONCENTRATIONSENSOR

| A device that senses or detects ion concentration such as water hardness. HISTORY: Added in IFC4.
| 水の硬度などのイオン濃度を感知または検出する装置

buildingSMART Data Dictionary

PSD-XML

- SubstanceDetected
  P_SINGLEVALUE / IfcLabel

  | SubstanceDetected: Identification of the substance that is being detected according to chemical formula. For example, calcium carbonate is 'CaCO3'
  | 対象物質: 検出されている物質の識別。
  | 대상 물질: 검출되는 물질의 식별.

- SetPointConcentration
  P_BOUNDEDVALUE / IfcIonConcentrationMeasure

  | SetPointConcentration: The ion concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
  | イオン濃度設定値: 感知されるイオン濃度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。
  | 이온 농도 설정: 감지되는 이온 농도. 세트 포인트 값을 넣으려면, IfcPropertyBoundedValue.SetPointValue를 사용하십시오.

Link to this page