#### 8.9.2.4 IfcElectricConductanceMeasure

IfcElectricConductanceMeasure is a measure of the electric conductance.

Usually measured in Siemens (S, 1/Ohm = A/V).

Type: REAL

> HISTORY New type in IFC2x.

XSD Specification:

<xs:simpleType name="IfcElectricConductanceMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
<xs:element name="IfcElectricConductanceMeasure-wrapper" nillable="true">
<xs:complexType>
<xs:simpleContent>
<xs:extension base="ifc:IfcElectricConductanceMeasure">
<xs:attributeGroup ref="ifc:instanceAttributes"/>
</xs:extension>
</xs:simpleContent>
</xs:complexType>
</xs:element>

EXPRESS Specification:

TYPE IfcElectricConductanceMeasure = REAL;
END_TYPE;

EXPRESS-G diagram

Link to this page