Timer Settings

1. Set time and day - press and hold CLOCK button press HOUR button to select current time -press MIN button to select current time – press WEEK button to select current day.

TO SET A PROGRAM

 1 Press TIMER button once the display will show “1 on “

1. Press WEEK button repeatedly until all the days of the week are displayed in the upper part of the display.
2. Press HOUR button to select the start time in hours.
3. Press MIN button to select start time in minutes.
4. Press TIMER button once the display will show “1 off”.
5. Press WEEK button repeatedly until all the days of the week are displayed in the upper part of the display.
6. Press HOUR button to select stop time in hours.
7. Press MIN button to select the stop time in minutes.

Repeat the above process to set additional feed times by pressing the TIMER button so the display window shows the next available program example “2 on” to set the second feed on time then press TIMER button to show “2 off” to set the second off time. You can then press TIMER button again to go to the third feed time “3 on” and repeat as many times needed to input the number of feeds required.

Final digital timer setting.

1 When connecting to a battery press the AUTO button which moves the arrow in the bottom right hand side of the display above “On” “Auto” “Off” press the AUTO button until the arrow is above the “Off” then press one more time so the arrow is above the “AUTO” you can now connect the battery.

To set the mechanical unit.

1 Set both left hand controls to “Off” by setting the toggle switch to “off” and turning the rotating knob completely anti clockwise until it will not turn any more.

2 Set both right hand controls as required the toggle can be set to either 3 or 5 seconds this setting will be the time the feeder will leave between dispensing food. The rotating knob can be set for time the food will be dispensed, by turning to a time in seconds the food will be emitted for this amount of time.

Example.

Set the toggle to 5 seconds and set the rotating knob to 5 seconds the unit will feed for 5 seconds with a 5 second gap then feed again for 5 seconds it will feed on and off for the duration of the power on time set in the digital timer so if the digital timer is set to start at 09.00 and stop at 09.01 it will run 5 seconds on and 5 seconds off during the one minute it is powered up.