Grob 103A					

VNE (Max Speed)	135 kts				
VA (Maneuvering)	92 kts				
Max Aero Tow	92 kts				
Max Airbrakes	135 kts				
					
	Solo	Dual			
VS (Stall Clean)	36 kts	41 kts			
VSO (Stall w/Airbrakes)	41 kts	46 kts			
VMIN	43 kts	46 kts	@ appx 130 ft/min		
VL/D	51 kts	57 kts	@ appx 36:1		

Load limit:					
@ VA 	+5.3 to -2.65				
@VNE	+4.0 to -1.5				
					
Max Operating Weight	1279 Lbs				
Current Empty Weight	866 Lbs				
Useful Load	413 Lbs				
Min Weight Solo	142 Lbs				
(Solo front seat only)					
Max seat weight	242 Lbs				
(Structural seat limit only)					
					
Max Crosswind	11 kts				
					
CSA recommended Landing	55 kts +1/2 wind factor