2 ea. Battery drills

2 ea. Screw driver set

2 ea. Diagonal cutting pliers

2 ea. 7 ½” Lineman pliers

2 ea. Wire stripper (10-26 g. stranded and 8-22 g. solid wire)

1 ea. Locking adjustable wrench

2 ea. C-clamp locking pliers

1 ea. Bi-metal groove joint pliers

1 ea. Set saw horses

1 ea. 10” Narrow London brick trowel

1 ea. Convex masonry jointer

1 ea. Modular spacing ruler

1 pr. Wood block line

1 ea. 18 oz. Brick hammer

1 ea. Mortar stand

1 ea. Wood chisel set

1 ea. Wonder bar pry bar

2 ea. Nail puller cats paw

1 ea. Hack saw with blade

1 ea. 24” Level

1 ea. 48” Level

2 ea. Rafter speed square

1 ea. Magnetic torpedo level

1 ea. Adjustable quick square

2 ea. Framing square

1 ea. Mason string

4 ea. Chalk reels with chalk

2 ea. Retractable utility knife with blades

2 ea. Straight cut aviation snips

4 ea. Framing hammer

4 ea. Finish hammer

1 ea. 8 ½” Wire stripper/crimper

1 pr. Brass stair gauges

1 ea. Long nose pliers with cutter

2 ea. Steel stud clamps

1 ea. Electrician tool belt

4 ea. Nail apron

4 ea. 25’ Tape measure

4 ea. Safety glasses

4 ea. Pair ear plugs

4 ea. Hard hats

1 ea. Tubing cutter

1 ea. 4 way pipe cleaner

1 ea. Torch with tank (propane or MAPP gas)

1 ea. 4 oz. Roll lead free solder

1 ea. Flux paste

1 ea. Flux brush

1 ea. ¾” Paddle bit

1 ea. ¾” Speed-bore bit

1 ea. Hole saw for 1 ½” Schedule 40 PVC

4 ea. Work gloves

2 ea. Magnetic bit holder with phillips bits

1 ea. 7 ¼” Circular saw with blade

1 ea. Reciprocating saw with wood and steel blades

4 ea. 50’ extension cord with ground

2 ea. 3 way extension cord splitter

2 ea. ½” Drill

1 ea. Mortar pan

1 ea. Mortar hoe

1 ea. Broom

1 ea. Dust pan or square point shovel

1 ea. Wrecking bar

2 ea. 6’ Step ladder

1 ea. Hand saw

1 ea. 12” Miter saw with blade

1 ea. 5 Gallon bucket

Note: Mortar boxes will be provided.