Specialty, Hauling Tanks

Flat Bottom tanks are designed to be the most rugged and durable utility transport tanks on the market. Unlike other tanks, Flat Bottom tanks provide all the strength you need for transporting liquids without the use of bands. Tanks should be mounted on flat surfaces with full length and width support.

[View Fitting Installation Guide for Specialty Hauling Tanks](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/FITTING%20INSTALLATION%20GUIDE%20FOR%20SPECIALTY%20HAULING%20TANKS.pdf)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Specialty, Flat Bottom** | | | | | | | | | |
| **Gallon Capacity** | **Width** | **Overall Height** | **Length** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** |
| 1600 Flat Bottom\* | 80" | 53" | 126" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [43143](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/1600%20Gallon%20Flat%20Bottom%20Tank.pdf) | B | [43167](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/1600%20Gallon%20Flat%20Bottom%20Tank.pdf) | B |
| 3180 Flat Bottom\* | 92" | 80" | 145" | 16"-(63485) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [44391](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/3180%20Gallon%20Flat%20Bottom%20Tank.pdf) | B | [44393](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/3180%20Gallon%20Flat%20Bottom%20Tank.pdf) | B |
| 4200 Flat Bottom\* | 96" | 85" | 180" | 16"-(63485) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [44972](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/4200%20Gallon%20Flat%20Bottom%20Tank.pdf) | B | [44974](https://www.norwesco.com/_site_components/uploads/pdfs/Specialty,%20Hauling/4200%20Gallon%20Flat%20Bottom%20Tank.pdf) | B |