Cone Bottom Tanks

Norwesco offers a full range of cone bottom tanks designed for a variety of applications. The conical bottoms enable quick and complete drainage. As with all Norwesco tanks, the cone bottom tanks are molded of rugged, high density polyethylene and are both impact and chemical resistant.

[View Fitting Installation Guide for Cone Bottom Tanks](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/FITTING%20INSTALLATION%20GUIDE%20FOR%20CONE%20BOTTOM%20TANKS.pdf)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Cone Bottom Tanks** | | | | | | | | | |
| **Gallon Capacity** | **Diameter** | **Overall Height** | **Slope** | **Fill Opening** | **Outlet/Drain Spec** | **Premium Weight Part No. White** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** |
| \*125 w/stand | 48" | 41" | 15° | 8"-(63480) | 2"-(60405) 2" street elbow (62199) | [43161](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/125%20Gallon%2015%20Degree%20Cone%20Tank%20With%20Containment.pdf) | B | NA | - |
| 160 | 36" | 52" | 45° | 16"-(63485) | 2"-(60405) | [43845](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/160%20Gallon%20x%2045%20Deg%20Cone%20Bottom%20Tank.pdf) | I | NA | - |
| \*175 w/stand | 43" | 49"/9"† | 30° | 16"-(63485) | 2"-(60405) 2" street elbow (62199) | [60113 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/175%20Gallon%20Cone%20Bottom%20Tank.pdf) [60113 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/175%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [60113 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/175_310%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Base.pdf) | B,C,D,E,F,I,L | NA | - |
| 300 | 48" | 56" | 45° | 16"-(63485) | 2"-(60405) | [43848](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/300%20Gallon%20X%2045%20Deg%20Cone%20Bottom%20Tank.pdf) | I | NA | - |
| \*300 w/stand | 49" | 61"/9"† | 30° | 16"-(63485) | 2"-(63683) | [62343 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/300%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [62343 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/300%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [62343 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/300-500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) | B,C,D,E,F,I,L | NA | - |
| \*310 w/stand | 43" | 72"/9"† | 30° | 8"-(63480) | 2"-(60405) 2" street elbow (62199) | [62441 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/310%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [62441 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/310%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [62441 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/175_310%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Base.pdf) | B,C,D,E,F,I,L | NA | - |
| 500 | 48" | 85" | 45° | 16"-(63485) | 2"-(60405) | [43850](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/500%20Gallon%20X%2045%20Deg%20Cone%20Bottom%20Tank.pdf) | I | NA | - |
| \*500 w/stand | 49" | 87"/9"† | 30° | 16"-(63485) | 2"-(63683) | [40289 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40289 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [40289 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/300-500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) | B,C,D,E,F,I,L | NA | - |
| 550 | 72" | 47" | 20° | 16"-(63485) | 2"-(63683) | 44647 | F,L | NA | - |
| \*550 w/stand | 73" | 57"/11"† | 20° | 16"-(63485) | 2"-(63683) | 44649 | F,L | NA | - |
| 750 | 72" | 56" | 20° | 16"-(63485) | 2"-(63683) | [40811](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/750%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank.pdf) | B,F,L | NA | - |
| \*750 w/stand | 73" | 67"/11"† | 20° | 16"-(63485) | 2"-(63683) | [40809 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/750%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank.pdf) [40809 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/750%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [40809 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/750-1050%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Stand.pdf) | B,F,L | NA | - |
| 1000 | 72" | 89" | 45° | 16"-(63485) | 2"-(63683) | [43852](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1000%20Gallon%20x%2045%20Deg%20Cone%20Bottom%20Tank.pdf) | B | NA | - |
| 1020 | 91" | 53" | 15° | 16"-(63485) | 2"-(63683) | [44341](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1020%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E | [44420](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1020%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E |
| 1050 | 72" | 75" | 20° | 16"-(63485) | 2"-(63683) | [40356](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1050%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank.pdf) | B,C,D,F,L | NA | - |
| \*1050 w/stand | 73" | 86"/11"† | 20° | 16"-(63485) | 2"-(63683) | [40359 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1050%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank.pdf) [40359 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1050%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [40359 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/750-1050%20Gallon%20x%2020%20Deg%20Cone%20Bottom%20Stand.pdf) | B,C,D,F,L | NA | - |
| **Cone Bottom Tanks** | | | | | | | | | |
| **Gallon Capacity** | **Diameter** | **Overall Height** | **Slope** | **Fill Opening** | **Outlet/Drain Spec** | **Premium Weight Part No. White** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** |
| 1320 | 91" | 64" | 15° | 16"-(63485) | 2"-(63683) | [44339](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1320%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E | [44422](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1320%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E |
| 1500 | 72" | 118" | 45° | 16"-(63485) | 2"-(63683) | [43854](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1500%20Gallon%20x%2045%20Deg%20Cone%20Bottom%20Tank.pdf) | B | NA | - |
| 1600 | 88" | 84" | 30° | 16"-(63485) | 2"-(63683) | [40817](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,C,D,F,L | [40819](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,C,D,F,L |
| \*1600 w/stand | 89" | 96"/11"† | 30° | 16"-(63485) | 2"-(63683) | [40813 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40813 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [40813 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Stand.pdf) | B,C,D,F,L | [40815 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40815 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) [40815 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/1600%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Stand.pdf) | B,C,D,F,L |
| 1720 | 91" | 78" | 15° | 16"-(63485) | 2"-(63683) | [44337](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1720%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E | [44424](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/1720%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E |
| 2500 | 91" | 108" | 15° | 16"-(63485) | 3"-(62299) | [43065](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | I | [43067](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | I |
| 2500 | 96" | 105" | 30° | 16"-(63485) | 2"-(63683) | [40066](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,C,D,L | [40129](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,C,D,L |
| \*2500 w/stand | 99" | 116"/10"† | 30° | 16"-(63485) | 2"-(63683) | [40672 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40672 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/2500-3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) [40672 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) | B,C,D,L | [40674 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40674 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/2500-3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) [40674 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/2500%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) | B,C,D,L |
| 3000 | 96" | 123" | 30° | 16"-(63485) | 2"-(63683) | [40170](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B | [40172](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B |
| \*3000 w/stand | 99" | 134"/10"† | 30° | 16"-(63485) | 2"-(63683) | [40797 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40797 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/2500-3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) [40797 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) | B | [40799 TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) [40799 STD](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/Cone%20Bottom%20Stands-poly/2500-3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Stand.pdf) [40799 UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank%20and%20Stand.pdf) | B |
| 3000 | 91" | 120" | 15° | 16"-(63485) | 3"-(62299) | [45141](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | E,F,I | [45242](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/3000%20Gallon%20X%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | E,F,I |
| 4950 | 102" | 159" | 15° | 16"-(63485) | 3"-(62299) | [45381](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/4950%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | X | [45383](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/4950%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | X |
| 5500 | 119" | 148" | 30° | 16"-(63485) | 3"-(62299) | [40549](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/5500%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J | [40316](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/5500%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J |
| 6000 | 102" | 189" | 10° | 16"-(63485) | 3"-(62299) | [43054](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/6000%20Gallon%20X%2010%20Deg%20Cone%20Bottom%20Tank.pdf) | L | [43056](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/6000%20Gallon%20X%2010%20Deg%20Cone%20Bottom%20Tank.pdf) | L |
| 6000 | 102" | 195" | 15° | 16"-(63485) | 3"-(62299) | [40931](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/6000%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J | [40933](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/6000%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J |
| 7500 | 141" | 149" | 30° | 16"-(63485) | 3"-(62299) | [40551](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/7500%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J | [40409](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/7500%20Gallon%20x%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,E,J |
| 10000 | 142" | 173" | 15° | 22"-(63679) | 3"-(62299) | [44459](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/10000%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,T | [44461](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/10000%20Gallon%20x%2015%20Deg%20Cone%20Bottom%20Tank.pdf) | B,T |
| 10000 | 141" | 190" | 30° | 16"-(63485) | 3"-(62299) | [44103](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/10000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,T | [44105](https://www.norwesco.com/_site_components/uploads/pdfs/Cone%20Bottom/10000%20Gallon%20X%2030%20Deg%20Cone%20Bottom%20Tank.pdf) | B,T |
| \* Polyethylene stand  †Distance from bottom of cone to ground | | | | | | | | | |