Inductor Tanks

Norwesco inductor tanks are suitable for mixing chemicals when filling a larger tank. The tanks feature a lid which threads directly into the fill-well of the tank to prevent the sloshing or leaking of contents during transport or application.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Inductor Tanks** | | | | | | | |
| **Gallon Capacity** | **Diameter** | **Overall Height** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** | **https://www.norwesco.com/_site_components/images/products/LSTInductor.jpg** |
| 15¤ | 19" | 23" | 8"-(63480) | 2"-(63481) | [60214](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/15%20Gallon%20x%2019D%20Inductor%20Tank.pdf) | A |
| 15¤ | 24" | 21" | 16"-(63485) | 2"-(63481) | [42064](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/15%20Gallon%20x%2024D%20Inductor%20Tank.pdf) | A |
| 30¤ | 24" | 28" | 16"-(63485) | 2"-(63481) | [42065](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/30%20Gallon%20Inductor%20Tank.pdf) | A |
| 35¤ | 23" | 29" | 8"-(63480) | 2"-(63481) | [45098](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/35%20Gallon%20Inductor%20Tank.pdf) | A |
| 40† | 27" | 34" | 16"-(63485) | See † | [44978](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/40%20Gallon%20Inductor%20Tank%20PN.pdf) | A |
| 60¤ | 31" | 32" | 16"-(63485) | 2"-(63481) | [62205](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/60%20Gallon%20x%2031D%20Inductor%20Tank.pdf) | A |
| 60 | 24" | 42" | 16"-(63485) | 2"-(63481) | [42066](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/60%20Gallon%20x%2024D%20Inductor%20Tank.pdf) | A |
| 65† | 27" | 43" | 16"-(63485) | See † | [44979](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/65%20Gallon%20Inductor%20Tank%20PN.pdf) | A |
| \*80 | 32" | 37" | 16"-(63485) | 2"-(63481) | [47190](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/80%20Gallon%20Inductor%20Tank.pdf) | A |
| † Full drain w/2" MPT molded into tank \*No stand available for this tank. | | | | | | | |

Inductor Tank Stands

Designed to provide necessary support for the inductor tank during use. Inductor stands are supplied with all necessary hardware.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Inductor Tank Stands** | | | | | |
| **Tank Size (Gallon)** | **Tank Part No.** | **A** | **B** | **Stand Part No.** | **https://www.norwesco.com/_site_components/images/products/IndctStand.jpg** |
| 15 x 19"D¤ | 60214 | 15-1/2" | 38" | [60313](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/15%20Gallon%20x%2019D%20Inductor%20Stand%20Steel.pdf) |
| 15 x 24"D¤ | 42064 | 13-1/2" | 36" | [63397](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/15-30-60%20x%2024D%20Inductor%20Stand%20Steel.pdf) |
| 30 x 24"D¤ | 42065 | 13-1/2" | 43" | [63397](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/15-30-60%20x%2024D%20Inductor%20Stand%20Steel.pdf) |
| 35 x 23"D¤ | 45098 | 15" | 44" | [65517](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/35%20Gallon%20Inductor%20Stand%20Steel.pdf) |
| 40 x 27"D-coming soon | 44978 |  |  | 64229 |
| 60 x 31"D¤ | 62205 | 14-1/2" | 47" | [62204](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/60%20Gallon%20x%2031D%20Inductor%20Stand%20Steel.pdf) |
| 60 x 24"D¤ | 42066 | 13-1/4" | 56" | [63397](https://www.norwesco.com/_site_components/uploads/pdfs/Inductor/Inductor%20Steel/15-30-60%20x%2024D%20Inductor%20Stand%20Steel.pdf) |
| 65 x 27"D-coming soon | 44979 |  |  | 64229 |