Elliptical Leg Tanks

This elliptical tank style is designed to provide the greatest capacity with the lowest center of gravity, making it the best design available for transporting larger volumes. Norwesco elliptical tanks feature molded-in legs that act as "baffles" to reduce sloshing and provide increased stability during transport.  The 2650 & 3250 include an internal baffle system.

All Norwesco elliptical leg tanks require full length bottom support as well as support bands.  The 1600 & 3180 flat bottoms require full length support but do not require bands.

[View Fitting Installation Guide for Elliptical Leg Tanks](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/FITTING%20INSTALLATION%20GUIDE%20FOR%20ELLIPTICAL%20LEG%20TANKS.pdf)

|  |
| --- |
| **Elliptical Leg Tanks** |
| **Gallon Capacity** | **Width** | **Overall Height** | **Length** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** | **PremiumWeightPart No.Black** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** | **Heavy Weight Part No. Black** | **Avail** |
| 135 | 36" | 26" | 56" | 8"-(63480) | 1 1/4"-(60403) | [44804](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/135%20Gallon%20Elliptical%20Leg%20Tank.pdf) | C,E,I,L | - | - | - | - |   |   |
| 235 | 40" | 32" | 66" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [44806](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/235%20Gallon%20Elliptical%20Leg%20Tank.pdf) | C,E,I,L | - | - | - | - |   |   |
| 335 | 48" | 33" | 71" | 16"-(63485) | 2"-(63481)2" siphon (60335) | [42339](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/335%20Gallon%20Elliptical%20Leg%20Tank.pdf) | C,E,L | - | -  | - | - | - | -  |
| 535 | 57" | 39" | 80" | 16"-(63485) | 2"-(63481)2" siphon (60335) | [42353](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/535%20Gallon%20Elliptcial%20Leg%20Tank.pdf) | C,E,L | - | -  | - | - | - | -  |
| 1035 | 79" | 54" | 89" | 16"-(63485) | 2"-(63683)2" siphon (60335) | [40191](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1035%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,F | - | -  | [40192](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1035%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,F | - | - |
| 1235 | 66" | 53" | 128" | 16"-(63485) | 2"-(63683)2" siphon (60335) | [40239](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1235%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B | - | - | - | - | - | -  |
| 1335 | 66" | 55" | 126" | 16"-(63485) | 2"-(63683)2" siphon (60335) | [42927](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1335%20%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C | - | -  | [42929](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1335%20%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C | - | -  |
| 1600 Flat Bottom\* | 80" | 53" | 126" | 16"-(63485) | 2"-(63683) | [43143](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1600%20Gallon%20Flat%20Bottom%20Elliptical%20Tank.pdf) | B | - | -  | [43167](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1600%20Gallon%20Flat%20Bottom%20Elliptical%20Tank.pdf) | B | - | -  |
| 1635 | 71" | 58" | 142" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [40387](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1635%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,D,E,F,L,T | [40602](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1635%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,D,E,F,L,T | [40388](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1635%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,D,E,F,L,T | [41890](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/1635%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,D,E,F,L,T |
| 2035 | 84" | 56" | 142" | 16"-(63485) | 2"-(63683)2" siphon (60335) | [40618-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20MN%20OK%20TX.pdf)[40618-CA-GA-OH-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20-CA-GA-OH-UT.pdf) | B,C,D,E,F,L,T | [40621-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20MN%20OK%20TX.pdf)[40621-CA-GA-OH-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20-CA-GA-OH-UT.pdf) | B,C,D,E,F,L,T  | [40623-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20MN%20OK%20TX.pdf)[40623-CA-GA-OH-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20-CA-GA-OH-UT.pdf) | B,C,D,E,F,L,T | [40775-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20MN%20OK%20TX.pdf)[40775-CA-GA-OH-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2035%20Gallon%20Elliptical%20Leg%20Tank%20-CA-GA-OH-UT.pdf) | B,C,D,E,F,L,T  |
| 2650 w/baffles | 88" | 82" | 122" | 22"\*\*\*-(63874) | 3"-(62299) 2" reducer(60330) 3" siphon (60327) | [45360](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2650%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [45364](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2650%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [45362](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2650%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [45366](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2650%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T |
| 2635 | 90" | 72" | 140" | 16"-(63485) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [40547-MN-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20MN%20TX.pdf)[40547-GA-OH-UT-CA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20-GA-OH-UT-CA.pdf) | B,C,D,F,L | [40751-MN-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20MN%20TX.pdf)[40751-GA-OH-UT-CA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20-GA-OH-UT-CA.pdf) | B,C,D,F,L | [40283-MN-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20MN%20TX.pdf)[40283-GA-OH-UT-CA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20-GA-OH-UT-CA.pdf) | B,C,D,F,L,T | [41294-MN-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20MN%20TX.pdf)[41294-GA-OH-UT-CA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/2635%20Gallon%20Elliptical%20Leg%20Tank%20-GA-OH-UT-CA.pdf) | B,C,D,F,L,T  |
| 3135 | 88" | 80" | 150" | 16"-(63485) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [40686-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-MN-OK-TX.pdf)[40686-OH-GA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-OH-GA.pdf)[40686-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-UT.pdf) | B,C,D,E,F,T | [40853-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-MN-OK-TX.pdf)[40853-OH-GA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-OH-GA.pdf)[40853-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-UT.pdf) | B,C,D,E,F,T  | [40688-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-MN-OK-TX.pdf)[40688-OH-GA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-OH-GA.pdf)[40688-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-UT.pdf) | B,C,D,E,F,T | [41417-MN-OK-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-MN-OK-TX.pdf)[41417-OH-GA](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-OH-GA.pdf)[41417-UT](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3135%20Gallon%20Elliptical%20Leg%20Tank%20-UT.pdf) | B,C,D,E,F,T  |
| 3180 Flat Bottom\* | 92" | 80" | 145" | 16"-(63485) | 3"/2"-(62299)-(63683) | [44391](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3180%20Gallon%20Flat%20Bottom%20Tank.pdf) | B | - |   | [44393](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3180%20Gallon%20Flat%20Bottom%20Tank.pdf) | B |   |   |
| 3250 w/baffles | 88" | 82" | 152" | 22"\*\*\*-(63874) | 3"-(62299)2" reducer (60330) 3" siphon (60327) | [44597](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3250%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [44601](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3250%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [44599](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3250%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T | [44603](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/3250%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,T |
| 4035 | 92" | 75" | 192" | 16"\*\*-(62532) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [41267](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/4035%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,L,T | [45394](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/4035%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,L,T | [41269](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/4035%20Gallon%20Elliptical%20Leg%20Tank.pdf) | B,C,L,T | [42011](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/4035%20Gallon%20Elliptical%20Leg%20Tank.pdf)  | B,C,L,T  |

\*Bands not available for this tank - not required.

\*\*16" hinged lid, Norwesco part number 62532.
\*\*\*22" hinged lid, Norwesco part number 63874.

Elliptical Leg Tanks, with the exception of the 1600 & 3180 Flat Bottoms, REQUIRE SUPPORT BANDS.

All Elliptical Leg Tanks REQUIRE FULL LENGTH SUPPORT.

Elliptical Leg Tank Bands

Norwesco bands are custom fabricated to support the Norwesco tanks and are galvanized for added corrosion protection. Whether using the tank in a stationary position or for transport, bands are necessary to ensure that the tank retains its shape and integrity.

|  |
| --- |
| **Elliptical Leg Tank Bands** |
| **Tank Size (Gallon)** | **A** | **B** | **C** | **Color of band foot** | **No. of Bands** | **Part No.** | **Avail** |  |  |  |  |  |
| 135 | 21" | 35"  | 39 11/16" | Galvanized | 2 required | [64164](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/135%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | C,E,I,L |  |  |  |  |  |
| 235 | 27 1/4"  | 38"  | 43 5/16" | Galvanized  | 2 required | [64165](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/235%20Gallon%20Elliptical%20Leg%20Tank.pdf) | C,E,I,L |  |  |  |  |  |
| 335 | 29" | 46 1/2" | 52 1/2" | Galvanized | 2 required | [63546](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/335%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | C,E,L |  |  |  |  |  |
| 535 | 35" | 55 1/2" | 61 1/2" | Galvanized | 2 required | [63547](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/535%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | C,E,L |  |  |  |  |  |
| 1035 | 47 1/4" | 77" | 83" | Yellow | 3 required | [60325](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/1035%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | B,C,F |  |  |  |  |  |
| 1235 | 47 3/4" | 64 3/4" | 70 3/4" | Dark Blue | 4 required | [60477](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/1235%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | B |  |  |  |  |  |
| 1335 | 49 3/4" | 63 1/2" | 69 1/2" | Blue | 3 required | [63642](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/1335%20Gallon%20Elliptical%20Leg%20Tank-1315%20Gallon%20Drainable%20Leg%20Tank%20Band%20PN.pdf) | B,C |  |  |  |  |  |
| 1635 | 50 3/8" | 68" | 74" | Brown | 4 required | [60586](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/1635%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | B,C,E,F,L,T |  |  |  |  |  |
| 1635 | 51 3/4"  | 68" | 74" | White | 4 required | [64191](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/1635%20Gallon%20Elliptical%20Leg%20Tank%20Band%20GA%20PN.pdf) | D |  |  |  |  |  |
| 2035 | 51 1/4" | 81 1/2" | 86 3/4" | Galvanized | 4 required | [62079](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2035%20Gallon%20Elliptical%20Leg%20Tank%20Band%20MN-OK-TX%20PN.pdf) | B,E,T |  |  |  |  |  |
| 2035 | 51 1/4" | 81 1/2" | 86 3/4" | Gold | 4 required | [63840](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2035%20Gallon%20Elliptical%20Leg%20Tank%20Band%20CA-GA-OH-UT%20PN.pdf) | C,D,F,L |  |  |  |  |  |
| 2635 | 65 1/4" | 87 1/2" | 94" | Galvanized | 4 required | [60353](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2635%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PM.pdf) | B,C,D,F,T |  |  |  |  |  |
| 2650 | 75 1/4" | 85 1/2" | 92" | Black | 3 required | [62097](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20GA-OH%20PN.pdf) | C |  |  |  |  |  |
| 2650 | 74 1/4" | 85 1/2" | 92" | Light Green | 3 required | [63620](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20MN-OK-TX-UT%20PN.pdf) | B,T |  |  |  |  |  |
| 3135 | 75 1/4" | 85 1/2" | 92" | Black | 4 required | [62097](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20GA-OH%20PN.pdf) | C,D |  |  |  |  |  |
| 3135 | 74 1/4" | 85 1/2" | 92" | Light Green | 4 required | [63620](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20MN-OK-TX-UT%20PN.pdf) | B,E,F,T |  |  |  |  |  |
| 3250 | 75 1/4" | 85 1/2" | 92" | Black | 4 required | [62097](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20GA-OH%20PN.pdf) | C |  |  |  |  |  |
| 3250 | 74 1/4" | 85 1/2" | 92" | Light Green | 4 required | [63620](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2650-3135-3250%20Gallon%20Elliptical%20Leg%20Tank%20Band%20MN-OK-TX-UT%20PN.pdf) | B,T |  |  |  |  |  |
| 4035 | 70 1/4" | 89 1/2" | 96" | Entire band painted Powder Gray. | 4 required | [62832](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/4035%20Gallon%20Elliptical%20Leg%20Tank%20Band%20PN.pdf) | B,C,L,T |  |  |  |  |  |

|  |
| --- |
| **Ladder** |
| **Description** | **Tank Size (Gallon)** | **Part No.** | **Avail** |
| Ladder-galvanized (optional) | 2635 & 3135 | [60354](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/2635-3135%20Gallon%20Elliptical%20Leg%20Tank%20Ladder%20PN.pdf) | B,C,D,E,F,T |
| Ladder-powder coated (optional) | 4035 | [63033](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/4035%20Gallon%20Elliptical%20Leg%20Tank%20Ladder%20PN.pdf) | B,C,L,T |
| \*Adaptor kit for ladder | 3135 | [62301](https://www.norwesco.com/_site_components/uploads/pdfs/Elliptical%20Leg/Elliptical%20Leg%20Steel/3135%20Gallon%20Elliptical%20Leg%20Tank%20Ladder%20Adapter%20PN.pdf) | B,C,D,E,F,T |

\*This kit is required when using ladder on the 3135 gallon tank.