**Richardson Inspection Services, LLC.**

2879 Mercer Butler Pike, Grove City, PA 16127 (724) 406-0031

**Summary Asbestos Requirements/Procedure Options for Demolitions and**

**Open Burning Requirements for Fire Fighting Instruction**

Part I: D.E.P. Bureau of Air Quality

 D.E.P. Contact: Laurie McNabb 724-656-3160 New Castle Office

 1. Certified Asbestos Inspector walk-thru

 A. Samples taken and analyzed

 B. Fills out Asbestos Abatement Form report and submits to appropriate agencies

 C. Abatement list to be processed with Certified Asbestos Abatement

 Contractor

 D. Submit application for open burning exception for fire fighting

 instruction 2700-PM-AQ002 - allow 45 days for process

 2. D.E.P. inspections possible upon application

 3. D.E.P. contact further noted that with a direct department contact request,

 including reference pictures from the fire department and municipality condemnation, the structure may be deemed unsanitary and unsafe (a detriment to community health and safety). The Department may at that

 time grant permission (after Department inspection) to skip the asbestos requirements and issue a permit to burn, just to remove the structure in a

 timely fashion.

Part II: Microbac Labs, Erie, PA

 Contact: Tim McLaughlin 814-825-8533

 1. Certified Asbestos Inspector—inspection approximately $200.00 and $25.00

 to process each suspected sample.

 2. Asbestos abatement via certified contractor (list available upon request)

 3. Certified Asbestos Inspector to fill out required D.E.P. forms notification - no re-inspection required.

 4. For demolition only—no certified inspection required—only “fryable” items (i.e., old pipe warp insulation) need removed. Should have a Certified Asbestos Abatement Contractor on site during demolition.

Rev 8/19