**Town of Sodus Harriman Park Floating Dock**

NYS Rout 14, Sodus Point NY

SPECIFICATIONS

January 19, 2022

RFQ for design, build and install floating dock on the north side of the ramp as depicted on the attached site plan.

1. Length to be the same as the fixed dock.
2. Width of dock six (6) feet.
3. Location as shown on site plan.
4. Dock to be properly anchored in the water. No attachment/s to the corrugated steel wall.
5. Land end to be anchored with ramp to facilitate different water levels.
6. Able to be used in water levels from 243.3 feet above sea level to 247.3. This is the same as the IJC Plan 58DD. With 243.3 being the chart datum and 247.3 the high limit. The existing fixed dock is at 249.81 feet.
7. Installed no later than May 15, 2022.
8. Quote to be valid until a grant is obtained but no longer than May 15, 2022, without reverification.
9. Decking to be of aluminum or composite material.