Fuel Policies

Type of Equipment      Type of Fuel to use

Aerator, WBH    Regular Gas
Air Compressor      Regular Gas
\*Air Compressor-Towable    Diesel

Bed edger, Trenchmaster Regular Gas
Blower - Backpack      Mixed (supplied by REQ)
Blower - WBH     Regular Gas
Brush mower - WBH     Regular Gas

Compactor, Medium     Regular Gas
Compactor, Small     Regular Gas
Compactor, Jumping Jack  Regular Gas
Cut off Saw, Handheld     Mixed (supplied by REQ)
Cut off Saw, WBH    Regular Gas
\*Forklift, Caterpillar   Propane
\*Forklift, All Terrain 6000  Diesel
\*Generator, Honda 2000   Regular Gas
\*Generator, Honda 5000     Regular Gas
\*Light Tower, Towable     Diesel
\*Log Splitter        Regular Gas
\*Manlift, All Terrain 46’ #3    Regular Gas/Propane
\*Manlift, All Terrain 46’ #4    Diesel
\*Mini Excavators    Diesel
Post Hole Digger 1 man     Regular Gas
Post Hole Digger 2 man     Regular Gas
Post Hole Digger, Towable Regular Gas
Pressure Washer 2700 psi    Regular Gas
Pressure Washer 3000 psi    Regular Gas
Pump, 2” Trash Pump   Regular Gas
Pump, 3” Diaphragm Mud Hog   Regular Gas
Pump, 3” Trash Pump      Regular Gas

\*Roller, Dynapac 3000lb Compactor Diesel
\*Skid Loader Tracks Diesel
\*Stump Grinder      Regular Gas
\*Tiller, WBH       Regular Gas
Tiller, Midtine Walk Behind Regular Gas
\*Tractor, John Deere 3038    Diesel

\*Trencher, WBH      Regular Gas
Trencher, 18”, Brave Regular Gas

\*Trencher, 24”, Barreto Wheel

If the item you are renting is listed above with an asterisk (\*) please refuel the machine before return. Otherwise, the fuel in the machine is yours to use. Please refill as needed to complete your job with the required fuel and you may return the machine empty.