**ADVANTAGES OF USING BLADDERS**

* Quality controlled, tested to twice the pressure exerted by water, by using air.
* Strong, durable, long lasting, with a patented corner system.
* Zero sun penetration – completely black inner surface.
* Zero algae growth.
* Zero change in water temperature – water sits against the top surface whether the unit is a quarter or three quarters empty.
* **Zero evaporation.**
* Zero toxicity (as in the case of sun eroded plastic tanks)
* UV stabilized reinforced PVC with a patented corner design – designed, patented and manufactured in South Africa since 2007.
* Easy to transport – a 200000L unit weighs 220kgs and can be thrown into the back of a car.
* Will last anything between 12-15 years, probably longer (warranty is for 10 years).
* Can be branded if required
* Easily repairable if ever needed.
* Easy to connect to downpipes, boreholes or irrigation systems.
* Can be supplied with fittings suitable for the correct connections to tanker trucks (Cam Lock fittings for example)
* Price per litre on size is not comparable to any other storage units – it is by far the cheapest method.
* Can be used for most fluids – water, fertilizer, diesel, transformer oil, cane juice, wine etc….PH charts for compatibility available on request.
* Can be custom made to sizes required.
* Full product back up, and continuous service excellence.

**STORAGE USES**

* WATER
* WINE
* FERTILIZER
* CANE JUICE
* BLOOD
* TRANSFORMER OIL
* DIESEL
* MOST AGRICULTURAL FLUIDS