LOCAL FACTORY/STREET STOCK CLASS
* GAS ONLY CLASS
• Driver must be 18 years of age or older with a valid driver's license.
• Drivers under 18 years of age may compete with a waiver signed by their legal guardian.
• Must have valid registration and insurance matching the VIN of the vehicle.
• Must have straps or chains for driveshaft loops preventing the driveshafts from hitting the ground if breakage occurs.
• No passengers allowed in vehicle — driver only.
• Must be driven onto the fairgrounds.
SAFETY
• Trucks cannot be gutted or stripped; must retain factory interior and exterior.
• Stock OEM front and rear bumpers are required — no ranch hands or fabricated bumpers. 
• Must have stock-style receiver hitch bolted in factory location — no fabricated hitches.
• Hitch height cannot exceed 26 inches and must have a clevis that is a 3.75 x 3 inch minimum.
• No front or rear blocks in suspension, along with no bound springs. (Must retain OEM spring pack.)
• No helper air bags allowed.
• Weights are not allowed anywhere in the vehicle.
• Truck must have OEM-style clutch; no slipper clutches, as well as a factory-style torque converter — no high stalls.
ENGINE
• Must have factory-style engine that matches make of the vehicle.
• No aftermarket camshafts.
• Must retain OEM style computer or ignition system.
• No aftermarket blocks or cylinder heads.
• Must be naturally aspirated — no power adders such as nitrous or turbo unless factory equipped.
• If the vehicle is carbureted, it must retain the factory intake manifold and carburetor.
• If the vehicle is fuel injected, it must retain the factory intake manifold and fuel injectors.
• The vehicle must have full exhaust that exits the rear of the vehicle with mufflers.
• Must run pump gas — no race gas or alcohol.
ALL DECISIONS CONCERNING TRUCK CLASSIFICATION AND
ELIGIBILITY WILL BE MADE BY THE TECH OFFICIALS 

