**A Message from**

**REPAIRS UNLIMITED**

**Millstone Township, N.J.**

**As the Winter Months approach, the following procedures and steps should take place to ensure that your snow blower and other small engine powered items you count on performing for you do just that… Perform in a Successful way.**

1. **Gas Shut-Off Valve: If you do not have a Gas Shut-Off Valve installed between the carburetor and Gas Tank, get one installed. During the Summer months with no valve installed, the ethanol in gas just contaminates the carburetor and plugs it up so it will not start when you need it. And if you have one installed already, USE it. After using your snow blower, etc., don’t shut it off electrically by pulling the key but by shutting the gas off to the carburetor. Leave it running outside of your garage for a few minutes until the carburetor runs out of gas and then with the next event, turn the Gas Shut-Off Valve On and fire it up. Success!!! . Repairs Unlimited offers the valves themselves for FREE, you just have to pay a minimal amount to have them installed.**
2. **Gas Stabilizer: During the off-season months or when your Lawn Tractor or Snow Blower sit for months in your garage or shed, always use a Gas Stabilizer in the Gas Tank as gas can go stale in 30 days. If you have stale gas or old gas in your gas tank, this alone will stop your piece of equipment from starting. So use a gas Stabilizer to keep the gas fresh and always turn off the gas valve so your unit is ready to go… Repairs Unlimited installs this in every unit that leaves here.**
3. **Dedicated Gas Container: If you count on your snow blower operating during the Winter months, and everyone does, buy a new gas can and write on it with a sharpie “Snow Blower Gas”. Why you ask, well if your lawn mower stops during the Summer because of dirt or water in the gas container, no biggie there, but if your Snow Blower quits while moving snow from your driveway and people cannot get to work, or school, that’s a problem.**