|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PORTABLE APPLIANCE TESTING (PAT) REPORT/CERTIFICATE** | | | | | | | | | | |
|  | | | |  | Certificate reference | | **Number INF1AMK** | | | |
|  | | | | | | | | | | |
| **DETAILS OF CLIENT/LANDLORD** | | | | | | | | | | |
|  | | | | | | | | | | |
| **Client/**  **Address:** | | INFINITY ENTERTAINMENT  22 Blackthorn Lane, Boston, Lincs, PE21 9BG | | | | | | | |  |
|  | | | | | | | | | | |
|  | | | | | | | | | | |
| **TEST EQUIPMENT DETAILS** | | | | | | | | | | |
| **Test Equipment used** | | | Seaward 100 Seaward Primetest 100 | | | **Serial Number** | | 344A910 | |  |
|  | | | | | | | | | | |
| **Tested by** | Anthony Kelham | | | | **Date** | 25/01/2019 | | **Retest Date** | 25/01/2020 25/11/2017 |  |
|  | | | | | | | | | | |
|  | | | | | | | | | | |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Serial Number** | Make and model | Location | Voltage (V) | Class **(1, 11, 111)** | Fuse rating (A) | Insulation resistance | Earth continuity | Plug, flex and body | OK to use ? |
| **00001** | LD Maui 28 Spk | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00002** | LD Maui 28 Spk | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00003** | DB Cromo Spk | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00004** | DB Cromo Spk | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00005** | Lanta Quad Beam | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00006** | Lanta Quad Beam | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00007** | QTX Hazer FX900 | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00008** | Nebula 400 Smoke M/C | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00009** | LantaG50 Laser | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00010** | Lanta G50 Laser | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00011** | Lanta Quad Beam | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00012** | Lanta Quad Beam | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00013** | Acme Marveled | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00014** | Acme Marveled | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00015** | IBM Monitor | Karaoke | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00016** | Equinox Triclops | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00017** | Stanton S450 CDJ | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00018** | Peavey 6ch Mixer | Karaoke | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00019** | Obey DMX Controller | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00020** | GoboSweeper | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00021** | GoboSweeper | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00022** | KamWireless Mic | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00023** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00024** | Kam Mixer | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00025** | Ext Lead 12 way | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00026** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00027** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00028** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00029** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00030** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00031** | Kam Wireless Mic | Rig 2 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00032** | 4 Way Ext Lead 5M | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00033** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00034** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **Serial Number** | Make and model | Location | Voltage (V) | Class **(1, 11, 111)** | 1 | 13 | Earth continuity | Plug, flex and body | OK to use ? |
| **00035** | IEC Lead | Rig 2 | 220 | 11 | 13 | Pass | Pass | Pass | YES |
| **00036** | IEC Lead | Rig 2 | 220 | 11 | 13 | Pass | Pass | Pass | YES |
| **00037** | IEC Lead | Rig 2 | 220 | 11 | 13 | Pass | Pass | Pass | YES |
| **00038** | Numark Mixer (USB) | Rig 2 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00039** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00040** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00041** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00042** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00043** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00044** | PAR Can (Uplighter) | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00045** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00046** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00047** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00048** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00049** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00050** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00051** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00052** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00053** | 5m 2 Way Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00054** | 5m Single Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00055** | 5m Single Ext | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00056** | 16 Way 5m Ext | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00057** | 24v AC Adapter | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00058** | 4 Way 5m Ext | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00059** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00060** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00061** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00062** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00063** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00064** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00065** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00066** | IEC Lead | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00067** | 5.3x AC Adapter | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00068** | 5.3x AC Adapter | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00069** | 24v AC Adapter | Rig 2 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00070** | 18v AC Adapter | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00071** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00072** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00073** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00074** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00075** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00076** | IEC Lead | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00077** | QTX Obsession | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00078** | Stanton S450 CDJ | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00079** | LantaG50 Laser | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00080** | Lanta G50 Laser | Rig 2 | 220 | 1 | 5 | Pass | Pass | Pass | YES |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Serial Number** | Make and model | Location | Voltage (V) | Class **(1, 11, 111)** | Fuse rating (A) | Insulation resistance | Earth continuity | Plug, flex and body | OK to use ? |
|  |  |  |  |  |  |  |  |  |  |
| **00081** | Kam Laserscan500 | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00082** | **LED Derby** | Rig 1 | 220 | 1 | 5 | Pass | Pass | Pass | YES |
| **00083** | KAM Mini Cluster | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00084** | KAM Mini Cluster | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00085** | AC Power Adapter | Rig 1 | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00086** | Power Dist 8 Way | Rig 2 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00087** | LD Maui 28 Spk | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00088** | LD Maui 28 Spk | Rig 1 | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00089** | Photo Booth | Photo Booth | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00090** | Photo Booth | Photo Booth | 220 | 1 | 13 | Pass | Pass | Pass | YES |
| **00091** | Toshiba Laptop | Photo Booth | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00092** | Toshiba Laptop | Photo Booth | 220 | 11 | 5 | Pass | Pass | Pass | YES |
| **00093** | 5m Ext Lead | Photo Booth | 220 | 1 | 13 | Pass | Pass | Pass | YES |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |