Weight and Balance: N32392
	
	Weight
	Arm
	Moment

	Empty
	1583.77
	87.37
	1583.77

	
Pilot
	
+_________________
	
80.5
	
+_________________

	
Passenger
	
+_________________
	
80.5
	
+_________________

	
Rear Seat
	
+_________________
	
118.1
	
+_________________

	
Baggage
	
+_________________
	
142.8
	
+_________________

	Zero Fuel Weight
(6 lbs./gal)
	
=_________________
	
CG:_______________
	
=__________________

	Usable Fuel
	+_________________
	______95_______
	+_________________

	
Ramp Weight
	
=_________________
	
             N/A
	
=_________________

	
Taxi Fuel
	
-________8_______
	
________95_______
	
-_________________

	
Takeoff Weight
	
=_________________
	
CG:_______________
	
=_________________

	
Fuel Burn
	
-_________________
	
________95_______
	
-__________________

	
Landing Weight 
	
=_________________
	
CG:_______________
	
=__________________


Max Gross: 2400 lbs.
Useful Load: 853.06
Formulas:  
· Weight X Arm= Moment
· Total Moment/ Total Weight= CG ( Center Gravity)
· Max Ramp Weight – Zero Fuel Weight = Usable Fuel Weight
· Fuel Weight/ 6= Fuel Gallons
· 100LL( Blue) Fuel Weights 6lbs./ Gal
· Oil Weights 7.5lbs/ gal 
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