Weight and Balance: N4982E
	
	Weight
	Arm
	Moment

	Empty
	1484.91
	38.71
	57483.1

	
Pilot
	
+_________________
	37
(34-46)
	
+_________________

	
Passenger
	
+_________________
	37
(34-46)
	
+_________________

	
Rear Seat
	
+_________________
	
73
	
+_________________

	
Baggage
	
+_________________
	
95
	
+_________________

	Zero Fuel Weight
(6 lbs./gal)
	
=_________________
	
CG:_______________
	
=__________________

	Usable Fuel

	
+_________________
	
_____ ___48_______
	
+_________________

	
Ramp Weight
	
=_________________
	
N/A
	
=_________________

	
Taxi Fuel
	
-__(-7lbs)_____
	
________48_______
	
-_________________

	
Takeoff Weight
	
=_________________
	
CG:_______________
	
=_________________

	Fuel Burn
	-_________________
	_______48_______
	-__________________

	Landing Weight
	=_________________
	CG:_______________
	=__________________






Max Gross: 2400 lbs.
Useful Load: 765
Formulas:  
· Weight X Arm= Moment
· Total Moment/ Total Weight= CG ( Center Gravity)
· Max Ramp Weight – Zero Fuel Weight = Usable Fuel Weight
· Fuel Weight/ 6= Fuel Gallons
· 100LL( Blue) Fuel Weights 6lbs./ Gal
· Oil Weights 7.5lbs/ gal 
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