|  |
| --- |
| Shanghai Hidong Intelligent Technology Co., Ltd.http：[www.hd-ebike.com](http://www.hd-ebike.com/)1 Jindi Plaza, Jiuting Town, Songjiang District, Shanghai, ChinaContact:bruce∣Tel:315 888 2138 ∣E-mail:info@hd-ebike.com |
| **Product picture** | **Performance** | **Main components** |
| 1192F689-BDD2-44ea-B220-6A88209B482B | **Max speed** | 25MILES/H | **Frame** | 6061 aluminum alloy suspension frame |
| **Range** | 40-50MILES | **Tyres** | KENDA 20\*4.0 |
| **Max load** | 120KG | **Rim** |  ALLOY RIM |
| **Net weight** | 36KG | **Front fork** | Aluminum alloy suspension with mechanical lockout |
| **Gross weight** | 40KG | **Front brake** | TEKTRO aries disc 180mm |
| **Dimension** |  | **Front brake** | TEKTRO aries disc 180mm |
| **Wheelbase** | 27.5"MM | **Rear Shock** | NONE |
| **Packing size** | 1520\*260\*850MM | **Rear derailleur** | SHIMANO ACERA |
| **Product Highlight** | **Container** |  | **Front derailleur** | N/A  |
| New lightweight folding |  |  | **Shifter** | SHIMANO  |
| **Climbing slope** | 8°-250Wmotor | 10°-350Wmotor | **Gears** | SHIMANO 14-28T |
| **Recharge cycles** | 7-8H 48V25A | **Hub** |  REAR HUB |
| **Charge time** | About 1000times | **Chainring Crank** | N/A |
| **Basic information** | **Electric system** | **Handlebar** | PROMAX ALLOY SSABK |
| **Model** | HD-006 | **Certificatio n** |  | **Motor: (Optional)** | 750W (rear hub)  | **Stem** | PROMAX MA-400 SSABK |
| **CN Name** | 灵动 | **Color: (Optional)** | WHITE/BLUE |  | N/A | **Seat post** | N/A |
| **EN Name** | agility | N/A |  | DC 51 malti function  |  | KMC Chain |
| **System NO.** | N/A | N/A | **Meter(LCD)** | **Chain** |
| **Factory** | Wuxi， Jiangsu | **Recreationa l sports style** |  | **Battery: (Optional)** | PowerPack 48V14Ah | **Chain wheel** | ALLOY SSABK |
| **spoke** | 13G-Stainless |  |  |  | SAMSUNG/LG | **Mudguard** | N/A |
| **Price: (Optional)** | FOB USD 860 |  |  | **Charger** | US standard 3.0 A smart charger | **Saddle** | SR |
| **Warranty：** | **Frame** | Lifetime | **Controller** | 48V multi-function integrated controller | **Pedal** |  ALLOY PREDAL |
| **Battery** | 2 years | **PAS** | sensor | **Headsets/B.B** | N/A |
| **Controlle r** | 2 years | **Throttle** | Adjustable uniform throttle | **Lighting** |  LED Headlight |
| **Parts** | 1 year | **Carrier** | NONE | **Reflector** | NEW LAN PMMA material |
|  |  |  |  |  |  |  | **Rear light** | SELLE ROYAL REAR SADDLE LIGHT |

