**HG-UV98**

**APRS firmware Update**

1, Turn off the radio.

2, Connect the supplied USB cable to the radio and computer.

3, Open up APRS firmware program.

4, Select the correct COM port.

5, Click “Update”.

6, Push and Hold “PF1” on HG-UV98,and turn of the radio.When see the “APRS update…” on the radio,then release “PF1”.

(you will see the progress bar is moving in the firmware update program)

7, When the progress bar is finish,turn off the radio,update is done)

