**SESC SITE PLAN SHEET**

**THE FOLLOWING ITEMS ARE REQUIRED BY PART 91 OF THE NATURAL RESOURCES AND ENVIRONMENTAL PROTECTION ACT 451 OF 1994 PRIOR TO OBTAINING A PERMIT**

**CHECK OFF ITEMS INCLUDED ON DRAWING, SITE PLAN AND/OR CONSTRUCTION SCHEDULE**

1) Final design plan detailing all items of work.

2) A map or site plan scaled down to no more than 200 feet per inch showing all predominant land features, physical structures, contour intervals and the distance from the earth change to drains, lakes or streams.

3) Description and location of all existing and proposed drainage and dewatering facilities, such as culverts.

4) Written soils description of the affected area.

PERCENTAGE OF EACH SOIL TYPE: SAND \_\_\_\_\_\_CLAY \_\_\_\_\_\_LOAM\_\_\_\_\_\_OTHER\_\_\_\_\_

5) Legal description of the site indicating legal ownership.

6) Description and location of the physical borders/limits of the proposed earth change.

7) Detailed schedule of each proposed earth change activity and the estimated date of completion.

(See attached SESC Installation & Construction schedule)

8) Description and the location of all existing and proposed drainage facilities (culvert, etc.)

9) Description and location for installing and removing all proposed temporary SESC measures.

10) Description and location of all proposed permanent SESC measures (seeding, riprap, etc.)

11) Written proposal for maintenance of permanent SESC measures, and the person responsible for continued maintenance. **Maintenance responsibilities are a part of any sale of exchange agreement for the land on which the permanent SESC measures are located.**

**A white sign with black text

AI-generated content may be incorrect.**